Technical documentation structure under Annex VII (Module A) of Regulation (EU) 2025/40	[image: ]
Technical documentation No. [TD-2026-0001]
Conformity assessment under Article 38 and Annex VII, Module A (internal production control). The structure follows Annex VII point 2(a) to (f) and adds the analysis and assessment of the risks of non-conformity required there. Delete the italic notes when filling in. One documentation per packaging type.
	Field
	Entry

	Manufacturer (Art. 3(1)(13))
	[Company, address, contact person]

	Packaging type / packaging unit
	[Name, type, article number, identifier under Art. 15(5)]

	Packaging category
	[Sales, grouped, transport, service or primary production packaging; single use or reusable; food contact yes/no]

	Related declaration of conformity
	[No. DoC-…, date]

	Version and date
	[Version 1.0, DD Month YYYY]

	Responsible
	[Name, position]

	Retention until
	[5 years from placing on the market, 10 years if reusable; Art. 15(3)]


0. Change history
Record every change of material, supplier, printing ink, adhesive or an underlying standard and check whether a new assessment is needed (Art. 15(4)).
	Version
	Date
	Change
	New assessment needed?

	
	
	
	

	
	
	
	

	
	
	
	


1. Applicable requirements
Annex VII point 2 requires the applicable requirements to be listed. Tick only requirements that apply when the packaging is placed on the market. As at September 2026 these are the following; the later requirements (Art. 6(2), 7, 9, 10, 12) are listed for information.
	Requirement
	Applicable
	Met
	Evidence in section / annex

	Art. 5(1)  Minimising substances of concern
	[yes]
	[yes/no]
	[6]

	Art. 5(4)  Pb, Cd, Hg, Cr VI combined max. 100 mg/kg
	[yes]
	[yes/no]
	[6.1, annexes …]

	Art. 5(5)  PFAS limits (food contact only)
	[yes/no]
	[yes/no]
	[6.2, annexes …]

	Art. 6(1)  Recyclability (general requirement)
	[yes]
	[yes/no]
	[7.1]

	Art. 11  Reusable packaging (reusable only)
	[yes/no]
	[yes/no]
	[7.3]

	Art. 15(5) and (6)  Identifier and manufacturer details on the packaging
	[yes]
	[yes/no]
	[3, annex figure]

	Art. 6(2)  Performance grades (from 1 January 2030 or later)
	no
	
	for information

	Art. 7  Recycled content (from 1 January 2030 or later)
	no
	
	for information

	Art. 9  Compostability (from 12 February 2028)
	no
	
	for information

	Art. 10  Minimisation, empty space (from 1 January 2030)
	no
	
	for information

	Art. 12  Harmonised labelling (from 12 August 2028 or later)
	no
	
	for information


2. Analysis and assessment of the risks of non-conformity
For each component, assess how likely the limits are to be exceeded and derive the appropriate evidence from this. Typical risk drivers: printing inks and varnishes, recycled material, metal parts, coatings, food contact.
	Component
	Risk
	Reasoning
	Evidence chosen

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


3. General description of the packaging and its intended use (point (a))
Packaging category, packed product, function, single use or reusable, food contact, labelling under Art. 15(5) and (6) (identifier, name, address, contact details), stating where it is applied.
[Description]
4. Designs, manufacturing drawings and materials of the components (point (b))
All components of the packaging unit including printing inks, varnishes, adhesives and labels. Drawings and specifications as annexes.
	Component
	Material / specification
	Mass (g)
	Supplier, article no.
	Annex (drawing, data sheet)

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


5. Explanations of drawings, schemes and operation (point (c))
[Explanations as far as needed for understanding]
6. Assessment of substance requirements under Article 5
6.1 Heavy metals (Art. 5(4))
The sum of lead, cadmium, mercury and chromium VI relates to the packaging including printing inks, varnishes and adhesives. State a test report or supplier declaration as the basis of evidence; test report where the risk is elevated.
	Component
	Sum (mg/kg)
	Basis of evidence
	Method / standard
	Annex, date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


6.2 PFAS in food contact (Art. 5(5))
Complete only if the packaging comes into contact with food. Limits: 25 ppb per individual PFAS, 250 ppb sum, 50 ppm total PFAS including polymeric PFAS. If total fluorine exceeds 50 mg/kg, evidence on the origin of the fluorine is required.
	Component
	Result
	Basis of evidence
	Method
	Annex, date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


6.3 Minimising substances of concern (Art. 5(1))
Briefly describe how substances of concern in material, emissions and waste are kept to a minimum, e.g. supplier declarations on REACH SVHC, choice of printing inks, avoiding certain additives.
[Description]
7. Qualitative description of the assessments under Articles 6, 10 and 11 (point (e))
7.1 Recyclability (Art. 6(1))
Until the performance grades under Art. 6(2) apply, the general requirement applies at the level of Directive 94/62/EC (Commission guidance C/2026/3702). Describe material combination, separability and disruptors; record material shares per component for the later assessment.
[Description]
7.2 Packaging minimisation (Art. 10)
Applies from 1 January 2030. Already useful today: document empty space and weight so the later assessment is traceable.
[Details, optional]
7.3 Reusable packaging (Art. 11)
Reusable packaging only: design for multiple rotations, cleaning, repair, labelling, system operation.
[Description or: not applicable, single-use packaging]
8. Standards, common specifications and technical specifications (point (d))
Harmonised standards for the PPWR are not yet listed in the Official Journal. Name the measurement and calculation methods applied; where no standard was applied, describe the solution chosen (Annex VII point 2(d)(v)).
	Standard / specification
	Applied for
	In full or in part

	CEN/CR 13695-1:2000
	Determination of heavy metal content
	[…]

	EN 13428:2004 (guidance, no presumption of conformity)
	Minimisation, recoverability
	[…]

	
	
	

	
	
	


9. Test reports and list of annexes (point (f))
	Annex
	Document
	Issuer
	Date

	1
	[Figure / drawing of the packaging unit]
	
	

	2
	[Supplier declaration heavy metals, component …]
	
	

	3
	[Test report …]
	
	

	
	
	
	

	
	
	
	

	
	
	
	


10. Release
With the release the manufacturer confirms that the manufacturing process and its monitoring ensure conformity with this documentation (Annex VII point 3) and that the declaration of conformity is based on this documentation.
Signed for and on behalf of:  	
Place and date of issue:  	
Name, position:  	
Signature:  	
Template provided by Polygon One GmbH, polygon-one.com. As at September 2026. Not legal advice. The manufacturer is responsible for content and issuance (Art. 39(4) Regulation (EU) 2025/40).	Page 
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